**HC-3208**

**2D Image Barcode Scanner**



**Features**

**●**Plug and play, not need any driver, easy to operate

**●**Use Complete dust-proof design to meet more applications

**●**Using latest decoder technology, can read all 1D and 2D barcodes

**●**Ergonomic design, comfortable operating sense, it is not easy to fatigue

**●**Supports to read screen barcodes, such as mobile phones and computers

**●**Widely used in Wechat pay and Alipay, can quickly realize the ID and QR codes

**●**l  Blue LED indicator and loud buzzer sound, can quick feedback reading recods

**Application area**

**Mainly used in commerce, health care, tobacco, some industries, etc.**

**HC-3208 Technical Specifications**

|  |  |
| --- | --- |
| Image(Pixels) | 640 pixels(H)\*480 pixels(v) |
| Light Source | Aiming: 617 nm LED; illumination:6500K LED |
| Scan Angle | Elevation angle 65°/Tilt angle 30°/Declination 55° |
| Host System Interfaces | TTL-232, USB (HID-KBW, Virtual serial Port) |
| Print Contrast | More than 25% |
| Read mode | Manual/Auto sensor |
| Visual Indicator | Blue LED Lights , Buzzer |
| DECODE CAPABILITY |  |
| 1D | 1D： UPC/EAN/JAN,UPC-A & UPC-E, EAN-8 & EAN-13, JAN-8 &JAN-13, ISBN/ISSN, Code 39 (with full ASCII), Codabar (NW7), Code 128 & EAN 128, Code 93, Interleaved 2 of 5 (ITF),Addendum 2 of 5, IATA Code, MSI/Plessy, China Postal Code,Code 32 (Italian Pharmacode), RSS 14, RSS Limited, RSS Expanded |
| 2D | 2D： QR Code, Data Matrix, PDF417,Aztec, Maxicode, etc. |
| PHYSICAL CHARACTERISTICS |  |
| Dimension | 173mm\*67mm\*94mm(L\*W\*H) |
| Package Box size | 505mm\*460mm\*380mm(L\*W\*H) |
| Weight | 220g (with cable) |
| Input Voltage | 5VDC±10% |
| Working Current | 170mA |